# Overview of S10 Remote Control

### Overview

The S10 model is AT&Ts standard and most widely used digital remote control. The S10 remote is used for Motorola AT&T UVERSE Digital TV box/TVs/VCRs/DVDs. Product Features Universal infrared remote control can control up to 3 additional devices Backlit to work well in low light conditions Convenient one button access to the U-verse features you use most often: Record, Guide, Menu and Video on Demand Technical Specifications Frequency: 36 kHz Battery Type: AA Alkaline Battery Quantity: Not included Operating Voltage: 2.2v to3.2v IC Memory Size: 64K Dimensions: W-58mm, L-192mm, H-30.88mm8.

The S10 is an infrared (IR) remote with a range up to 30' (The range quoted is calculated based on an unobstructed line of sight test under optimum conditions. Actual range will vary depending on conditions, and can be less than the maximum possible. Your actual range will be limited by several factors including, but not Limited to: battery strength, infrared interference, and obstructions.). The S10 is a intended for use only with AT&Ts U-verse TV receivers and DVRs. The remote control's universal features may not be compatible with all devices or capable of accepting every programming code or operating every function for all devices.